//*************************************************************//

//           ATA Tool Version: SP_ATA_Tool_v2.1640.00

//*************************************************************//

2017/03/24/14/29/21/921 Get PM CommModule ok.

2017/03/24/14/29/22/106 Init state index = 1, wait for preloader com port 6.

2017/03/24/14/29/25/532 Find preloader com port OK, start booting target into factory mode.

2017/03/24/14/29/25/894 Enter factory mode ok, set state index = 2

2017/03/24/14/29/25/894 Searching kernel com port 12.

2017/03/24/14/29/36/474 Find kernel com port ok, set state index = 3

2017/03/24/14/29/36/474 GetCommModule ok.

2017/03/24/14/29/36/474 Send Start Command (AT+START) start.

2017/03/24/14/29/36/474 Send start command 1.

2017/03/24/14/29/36/909 Send start command 2.

2017/03/24/14/29/37/076 Get response pass, OK!

2017/03/24/14/29/37/076 Send Start Command (AT+START) ok.

2017/03/24/14/29/37/076 Send request flag command.

2017/03/24/14/29/37/385 Get flag from target OK!

2017/03/24/14/29/37/385 flag sequence from target are:ITEM_MAIN_CAMERA,ITEM_MAIN2_CAMERA,ITEM_SUB_CAMERA,ITEM_STROBE,ITEM_GPS,ITEM_NFC,ITEM_FM,ITEM_FMTX,ITEM_FLASH,ITEM_MEMCARD,ITEM_RTC,ITEM_LCD,ITEM_LCM,ITEM_BACKLIGHT,ITEM_LED,ITEM_LOOPBACK,ITEM_LOOPBACK1,ITEM_LOOPBACK2,ITEM_LOOPBACK3,ITEM_BT,ITEM_WIFI,ITEM_KEYS,ITEM_LOOPBACK_PHONEMICSPK,ITEM_WAVEPLAYBACK,ITEM_ACOUSTICLOOPBACK,ITEM_GSENSOR,ITEM_GS_CALI,ITEM_MSENSOR,ITEM_ALSPS,ITEM_HEADSET,ITEM_HEADSET_DEBUG,ITEM_USB,ITEM_OTG,ITEM_CLRFLASH,ITEM_CHARGER,ITEM_TOUCH,ITEM_TOUCH_AUTO,ITEM_SIM,ITEM_VIBRATOR,ITEM_RECEIVER,ITEM_RECEIVER_DEBUG,ITEM_SIMCARD,ITEM_IDLE,ITEM_TVOUT,ITEM_JOGBALL,ITEM_OFN,ITEM_MATV_NORMAL,ITEM_MATV_AUTOSCAN,ITEM_MUI_TEST,ITEM_FULL_TEST,ITEM_ITEM_TEST,ITEM_AUTO_TEST,ITEM_DEBUG_TEST,ITEM_VERSION,ITEM_REPORT,ITEM_UPDATE,ITEM_REBOOT,ITEM_BAROMETER,ITEM_GYROSCOPE,ITEM_GYROSCOPE_CALI,ITEM_SPK_OC,ITEM_SIGNALTEST,ITEM_CMMB,ITEM_EMMC,ITEM_EMI,ITEM_CLREMMC,ITEM_HDMI,ITEM_RECEIVER_PHONE,ITEM_HEADSET_PHONE,ITEM_LOOPBACK_PHONEMICSPK_PHONE,ITEM_VIBRATOR_PHONE,ITEM_MICBIAS,ITEM_CUSTOM_START,ITEM_CUSTOM_STOP,ITEM_CUSTOM_REQUESTDATA,ITEM_CUSTOM_VERSION,ITEM_CUSTOM_READBARCODE,ITEM_CUSTOM_WRITEBARCODE,ITEM_CUSTOM_CAMERADATA,ITEM_CUSTOM_PROPERTY,ITEM_RF_TEST,ITEM_UNIVERSAL_ANT_TEST,ITEM_HOTKNOT,ITEM_BTS,ITEM_EXT_BUCK,ITEM_EXT_VBAT_BOOST,ITEM_SPEAKER_MONITOR,ITEM_SPEAKER_MONITOR_SET_TMP,ITEM_RF_C2K_TEST,ITEM_USB_TYPEC,ITEM_IRTX_LED_TEST,ITEM_HEART_MONITOR,ITEM_EFUSE,ITEM_MAIN_LENS,ITEM_MAIN2_LENS,ITEM_SUB_LENS,ITEM_FINGERPRINT_TEST,ITEM_HUMIDITY,ITEM_CUSTOM_REQUESTFLAG,ITEM_MAX_IDS,

2017/03/24/14/29/37/385 Start parsing...

2017/03/24/14/29/37/385 Parse flag success,total number is:77921224

2017/03/24/14/29/37/385 In function ConvertToPCItemSequence(),convert flag sequence to g_convert_flag_item,total number is:100

2017/03/24/14/29/37/385 target_flag_sequence[0]= ITEM_MAIN_CAMERA

2017/03/24/14/29/37/385 target_flag_sequence[1]= ITEM_MAIN2_CAMERA

2017/03/24/14/29/37/385 target_flag_sequence[2]= ITEM_SUB_CAMERA

2017/03/24/14/29/37/385 target_flag_sequence[3]= ITEM_STROBE

2017/03/24/14/29/37/385 ITEM_STROBE not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/385 target_flag_sequence[4]= ITEM_GPS

2017/03/24/14/29/37/385 target_flag_sequence[5]= ITEM_NFC

2017/03/24/14/29/37/385 ITEM_NFC not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/385 target_flag_sequence[6]= ITEM_FM

2017/03/24/14/29/37/385 target_flag_sequence[7]= ITEM_FMTX

2017/03/24/14/29/37/385 target_flag_sequence[8]= ITEM_FLASH

2017/03/24/14/29/37/386 target_flag_sequence[9]= ITEM_MEMCARD

2017/03/24/14/29/37/386 target_flag_sequence[10]= ITEM_RTC

2017/03/24/14/29/37/386 target_flag_sequence[11]= ITEM_LCD

2017/03/24/14/29/37/386 target_flag_sequence[12]= ITEM_LCM

2017/03/24/14/29/37/386 target_flag_sequence[13]= ITEM_BACKLIGHT

2017/03/24/14/29/37/386 ITEM_BACKLIGHT not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/386 target_flag_sequence[14]= ITEM_LED

2017/03/24/14/29/37/386 target_flag_sequence[15]= ITEM_LOOPBACK

2017/03/24/14/29/37/386 target_flag_sequence[16]= ITEM_LOOPBACK1

2017/03/24/14/29/37/386 target_flag_sequence[17]= ITEM_LOOPBACK2

2017/03/24/14/29/37/386 target_flag_sequence[18]= ITEM_LOOPBACK3

2017/03/24/14/29/37/386 target_flag_sequence[19]= ITEM_BT

2017/03/24/14/29/37/386 target_flag_sequence[20]= ITEM_WIFI

2017/03/24/14/29/37/386 target_flag_sequence[21]= ITEM_KEYS

2017/03/24/14/29/37/386 target_flag_sequence[22]= ITEM_LOOPBACK_PHONEMICSPK

2017/03/24/14/29/37/386 target_flag_sequence[23]= ITEM_WAVEPLAYBACK

2017/03/24/14/29/37/386 target_flag_sequence[24]= ITEM_ACOUSTICLOOPBACK

2017/03/24/14/29/37/386 target_flag_sequence[25]= ITEM_GSENSOR

2017/03/24/14/29/37/386 target_flag_sequence[26]= ITEM_GS_CALI

2017/03/24/14/29/37/386 target_flag_sequence[27]= ITEM_MSENSOR

2017/03/24/14/29/37/386 target_flag_sequence[28]= ITEM_ALSPS

2017/03/24/14/29/37/386 target_flag_sequence[29]= ITEM_HEADSET

2017/03/24/14/29/37/386 target_flag_sequence[30]= ITEM_HEADSET_DEBUG

2017/03/24/14/29/37/387 target_flag_sequence[31]= ITEM_USB

2017/03/24/14/29/37/387 ITEM_USB not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/387 target_flag_sequence[32]= ITEM_OTG

2017/03/24/14/29/37/387 target_flag_sequence[33]= ITEM_CLRFLASH

2017/03/24/14/29/37/387 ITEM_CLRFLASH not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/387 target_flag_sequence[34]= ITEM_CHARGER

2017/03/24/14/29/37/387 target_flag_sequence[35]= ITEM_TOUCH

2017/03/24/14/29/37/387 target_flag_sequence[36]= ITEM_TOUCH_AUTO

2017/03/24/14/29/37/387 target_flag_sequence[37]= ITEM_SIM

2017/03/24/14/29/37/387 target_flag_sequence[38]= ITEM_VIBRATOR

2017/03/24/14/29/37/387 target_flag_sequence[39]= ITEM_RECEIVER

2017/03/24/14/29/37/387 target_flag_sequence[40]= ITEM_RECEIVER_DEBUG

2017/03/24/14/29/37/387 target_flag_sequence[41]= ITEM_SIMCARD

2017/03/24/14/29/37/387 target_flag_sequence[42]= ITEM_IDLE

2017/03/24/14/29/37/387 target_flag_sequence[43]= ITEM_TVOUT

2017/03/24/14/29/37/387 target_flag_sequence[44]= ITEM_JOGBALL

2017/03/24/14/29/37/387 ITEM_JOGBALL not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/387 target_flag_sequence[45]= ITEM_OFN

2017/03/24/14/29/37/387 ITEM_OFN not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/387 target_flag_sequence[46]= ITEM_MATV_NORMAL

2017/03/24/14/29/37/387 target_flag_sequence[47]= ITEM_MATV_AUTOSCAN

2017/03/24/14/29/37/387 target_flag_sequence[48]= ITEM_MUI_TEST

2017/03/24/14/29/37/387 ITEM_MUI_TEST not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/387 target_flag_sequence[49]= ITEM_FULL_TEST

2017/03/24/14/29/37/387 ITEM_FULL_TEST not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/388 target_flag_sequence[50]= ITEM_ITEM_TEST

2017/03/24/14/29/37/388 ITEM_ITEM_TEST not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/388 target_flag_sequence[51]= ITEM_AUTO_TEST

2017/03/24/14/29/37/388 ITEM_AUTO_TEST not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/388 target_flag_sequence[52]= ITEM_DEBUG_TEST

2017/03/24/14/29/37/388 ITEM_DEBUG_TEST not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/388 target_flag_sequence[53]= ITEM_VERSION

2017/03/24/14/29/37/388 target_flag_sequence[54]= ITEM_REPORT

2017/03/24/14/29/37/388 ITEM_REPORT not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/388 target_flag_sequence[55]= ITEM_UPDATE

2017/03/24/14/29/37/388 ITEM_UPDATE not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/388 target_flag_sequence[56]= ITEM_REBOOT

2017/03/24/14/29/37/388 ITEM_REBOOT not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/388 target_flag_sequence[57]= ITEM_BAROMETER

2017/03/24/14/29/37/388 target_flag_sequence[58]= ITEM_GYROSCOPE

2017/03/24/14/29/37/388 target_flag_sequence[59]= ITEM_GYROSCOPE_CALI

2017/03/24/14/29/37/388 target_flag_sequence[60]= ITEM_SPK_OC

2017/03/24/14/29/37/388 target_flag_sequence[61]= ITEM_SIGNALTEST

2017/03/24/14/29/37/388 target_flag_sequence[62]= ITEM_CMMB

2017/03/24/14/29/37/388 target_flag_sequence[63]= ITEM_EMMC

2017/03/24/14/29/37/388 target_flag_sequence[64]= ITEM_EMI

2017/03/24/14/29/37/388 ITEM_EMI not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/388 target_flag_sequence[65]= ITEM_CLREMMC

2017/03/24/14/29/37/389 ITEM_CLREMMC not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/389 target_flag_sequence[66]= ITEM_HDMI

2017/03/24/14/29/37/389 target_flag_sequence[67]= ITEM_RECEIVER_PHONE

2017/03/24/14/29/37/389 target_flag_sequence[68]= ITEM_HEADSET_PHONE

2017/03/24/14/29/37/389 target_flag_sequence[69]= ITEM_LOOPBACK_PHONEMICSPK_PHONE

2017/03/24/14/29/37/389 target_flag_sequence[70]= ITEM_VIBRATOR_PHONE

2017/03/24/14/29/37/389 target_flag_sequence[71]= ITEM_MICBIAS

2017/03/24/14/29/37/389 target_flag_sequence[72]= ITEM_CUSTOM_START

2017/03/24/14/29/37/389 ITEM_CUSTOM_START not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/389 target_flag_sequence[73]= ITEM_CUSTOM_STOP

2017/03/24/14/29/37/389 ITEM_CUSTOM_STOP not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/389 target_flag_sequence[74]= ITEM_CUSTOM_REQUESTDATA

2017/03/24/14/29/37/389 ITEM_CUSTOM_REQUESTDATA not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/389 target_flag_sequence[75]= ITEM_CUSTOM_VERSION

2017/03/24/14/29/37/389 target_flag_sequence[76]= ITEM_CUSTOM_READBARCODE

2017/03/24/14/29/37/389 target_flag_sequence[77]= ITEM_CUSTOM_WRITEBARCODE

2017/03/24/14/29/37/389 target_flag_sequence[78]= ITEM_CUSTOM_CAMERADATA

2017/03/24/14/29/37/389 ITEM_CUSTOM_CAMERADATA not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/389 target_flag_sequence[79]= ITEM_CUSTOM_PROPERTY

2017/03/24/14/29/37/389 ITEM_CUSTOM_PROPERTY not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/389 target_flag_sequence[80]= ITEM_RF_TEST

2017/03/24/14/29/37/389 target_flag_sequence[81]= ITEM_UNIVERSAL_ANT_TEST

2017/03/24/14/29/37/389 target_flag_sequence[82]= ITEM_HOTKNOT

2017/03/24/14/29/37/389 ITEM_HOTKNOT not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/389 target_flag_sequence[83]= ITEM_BTS

2017/03/24/14/29/37/390 target_flag_sequence[84]= ITEM_EXT_BUCK

2017/03/24/14/29/37/390 target_flag_sequence[85]= ITEM_EXT_VBAT_BOOST

2017/03/24/14/29/37/390 ITEM_EXT_VBAT_BOOST not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/390 target_flag_sequence[86]= ITEM_SPEAKER_MONITOR

2017/03/24/14/29/37/390 ITEM_SPEAKER_MONITOR not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/390 target_flag_sequence[87]= ITEM_SPEAKER_MONITOR_SET_TMP

2017/03/24/14/29/37/390 ITEM_SPEAKER_MONITOR_SET_TMP not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/390 target_flag_sequence[88]= ITEM_RF_C2K_TEST

2017/03/24/14/29/37/390 ITEM_RF_C2K_TEST not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/390 target_flag_sequence[89]= ITEM_USB_TYPEC

2017/03/24/14/29/37/390 target_flag_sequence[90]= ITEM_IRTX_LED_TEST

2017/03/24/14/29/37/390 ITEM_IRTX_LED_TEST not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/390 target_flag_sequence[91]= ITEM_HEART_MONITOR

2017/03/24/14/29/37/390 ITEM_HEART_MONITOR not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/390 target_flag_sequence[92]= ITEM_EFUSE

2017/03/24/14/29/37/390 ITEM_EFUSE not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/390 target_flag_sequence[93]= ITEM_MAIN_LENS

2017/03/24/14/29/37/390 ITEM_MAIN_LENS not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/390 target_flag_sequence[94]= ITEM_MAIN2_LENS

2017/03/24/14/29/37/390 ITEM_MAIN2_LENS not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/390 target_flag_sequence[95]= ITEM_SUB_LENS

2017/03/24/14/29/37/390 ITEM_SUB_LENS not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/390 target_flag_sequence[96]= ITEM_FINGERPRINT_TEST

2017/03/24/14/29/37/390 target_flag_sequence[97]= ITEM_HUMIDITY

2017/03/24/14/29/37/391 target_flag_sequence[98]= ITEM_CUSTOM_REQUESTFLAG

2017/03/24/14/29/37/391 ITEM_CUSTOM_REQUESTFLAG not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/391 target_flag_sequence[99]= ITEM_MAX_IDS

2017/03/24/14/29/37/391 ITEM_MAX_IDS not defined test item in this tool,convert to E_TEST_ITEM_COUNT.

2017/03/24/14/29/37/391 Get and parse target side's flag sequence successful!Using flag sequence get from target

2017/03/24/14/29/37/425 Sleep 0 second before test.

2017/03/24/14/29/37/425 Init test item object.

2017/03/24/14/29/37/425 Start Testing items:



2017/03/24/14/29/37/425 Start test items.

2017/03/24 14:29:37.425 ====== [OTG] Start Test ======

2017/03/24 14:29:37.740 Control target enter OTG mode....

2017/03/24 14:29:39.441 Close kernel com port handle of Target....

2017/03/24/14/29/39/441 Release target comm handle.

2017/03/24 14:29:39.543 Disconnect USB Vbus to disable charging.

2017/03/24 14:29:39.590 Pull down OTG Pin to enable OTG.

2017/03/24 14:29:47.715 [OK] Power measure voltage sub : 5197 .

2017/03/24 14:29:47.715 [1] Measure voltage result: 5.197 v

2017/03/24 14:29:49.502 [OK] Power measure voltage sub : 5206 .

2017/03/24 14:29:49.502 [2] Measure voltage result: 5.206 v

2017/03/24 14:29:51.293 [OK] Power measure voltage sub : 5214 .

2017/03/24 14:29:51.293 [3] Measure voltage result: 5.214 v

2017/03/24 14:29:51.293 [OTG]Measure voltage final result: 5.214 v

2017/03/24 14:29:54.293 Pull up OTG Pin to disable OTG.

2017/03/24 14:29:56.432 Reconnect USB Vbus.

2017/03/24 14:29:59.583 Wait and open kernel com port of target.

2017/03/24/14/29/59/583 Init state index = 2, wait for kernel com port 12.

2017/03/24/14/29/59/593 Find kernel com port ok, set state index = 3

2017/03/24/14/29/59/593 GetCommModule ok.

2017/03/24 14:30:02.663 [OK] Test finished

2017/03/24 14:30:02.664 Time cost: 25.239 second

2017/03/24 14:30:02.665 ====== [OTG] End Test ======



2017/03/24 14:30:02.984 GetATAData data size: 1688.

2017/03/24 14:30:02.984 GetATAData sp_ata_data size: 1684.

2017/03/24 14:30:02.984 GetATAData sp_ata_data_old size: 1192.

2017/03/24 14:30:02.984 GetATAData sp_ata_data_old_ex size: 1248.

2017/03/24/14/30/02/984 [OK] Request data successfully.

2017/03/24/14/30/02/995 OTG,1,OK,E_ATADLL_RESULT_SUCCESS

2017/03/24 14:30:02.998 ====== [Charger] Start Test ======

2017/03/24 14:30:05.055 [Charger ERROR]Charger Test fail from target.

2017/03/24 14:30:05.058 Test Error:E_ATADLL_RESULT_FAILED,Error code is 1



2017/03/24 14:30:05.058 Time cost: 2.060 second

2017/03/24 14:30:05.058 ====== [Charger] End Test ======



2017/03/24 14:30:05.368 GetATAData data size: 1688.

2017/03/24 14:30:05.368 GetATAData sp_ata_data size: 1684.

2017/03/24 14:30:05.368 GetATAData sp_ata_data_old size: 1192.

2017/03/24 14:30:05.368 GetATAData sp_ata_data_old_ex size: 1248.

2017/03/24/14/30/05/368 [OK] Request data successfully.

2017/03/24/14/30/05/373 Charger,1,Fail,E_ATADLL_RESULT_FAILED

2017/03/24 14:30:05.374 ====== [ADC] Start Test ======

2017/03/24 14:30:06.820 [ADC OK] Power measure Samples : 3958 .

2017/03/24 14:30:06.820 [OK] Switch sample to voltage is : 3.958 V.

2017/03/24 14:30:08.906 [ADC ERROR]Target ADC test fail.

2017/03/24 14:30:08.912 Test Error:E_ATADLL_RESULT_FAILED,Error code is 1



2017/03/24 14:30:08.912 Time cost: 3.537 second

2017/03/24 14:30:08.912 ====== [ADC] End Test ======



2017/03/24 14:30:09.221 GetATAData data size: 1688.

2017/03/24 14:30:09.221 GetATAData sp_ata_data size: 1684.

2017/03/24 14:30:09.221 GetATAData sp_ata_data_old size: 1192.

2017/03/24 14:30:09.221 GetATAData sp_ata_data_old_ex size: 1248.

2017/03/24/14/30/09/221 [OK] Request data successfully.

2017/03/24/14/30/09/227 ADC,1,Fail,E_ATADLL_RESULT_FAILED

2017/03/24 14:30:09.228 ====== [BTS] Start Test ======

2017/03/24 14:30:14.434 [OK] BTS test stop measure temperature.

2017/03/24 14:30:14.435 Time cost: 5.207 second

2017/03/24 14:30:14.435 ====== [BTS] End Test ======



2017/03/24 14:30:14.746 GetATAData data size: 1688.

2017/03/24 14:30:14.746 GetATAData sp_ata_data size: 1684.

2017/03/24 14:30:14.746 GetATAData sp_ata_data_old size: 1192.

2017/03/24 14:30:14.746 GetATAData sp_ata_data_old_ex size: 1248.

2017/03/24/14/30/14/746 [OK] Request data successfully.

2017/03/24/14/30/14/749 BTS,1,OK,E_ATADLL_RESULT_SUCCESS

2017/03/24/14/30/14/752 Start to request test result data.

2017/03/24 14:30:15.085 GetATAData data size: 1688.

2017/03/24 14:30:15.085 GetATAData sp_ata_data size: 1684.

2017/03/24 14:30:15.085 GetATAData sp_ata_data_old size: 1192.

2017/03/24 14:30:15.085 GetATAData sp_ata_data_old_ex size: 1248.

2017/03/24/14/30/15/085 [OK] Request data successfully.

2017/03/24/14/30/15/085 

2017/03/24/14/30/15/085 [Charger] Current: 0.000 mA

2017/03/24/14/30/15/085 Battery temparature: 0

2017/03/24/14/30/15/085 

2017/03/24/14/30/15/085 [ADC] Voltage: 3.893 V

2017/03/24/14/30/15/085 

2017/03/24/14/30/15/085 [BTS] sensor_name:  mtktsAP, temperature: 29.0

2017/03/24/14/30/15/085 [BTS] sensor_name:  mtktsbtsmdpa, temperature: 24.0

2017/03/24/14/30/15/085 

2017/03/24/14/30/15/385 OTG result pass.



2017/03/24/14/30/15/386 Update ATA test flag into Barcode start.

2017/03/24 14:30:15.386 Update ATA test flag (f) into barcode[59].

2017/03/24 14:30:16.959 Read original barcode ok: unknown                                                    f

2017/03/24 14:30:16.959 Write new barcode: unknown                                                    f

2017/03/24 14:30:16.959 Wirte command to target: AT+BARCODE=0,1,"unknown                                                    f"


2017/03/24 14:30:20.094 Write new barcode ok.

2017/03/24 14:30:20.594 Read barcode again to check if write succesfully.

2017/03/24 14:30:22.041 New readed barcode is: unknown                                                    f

2017/03/24 14:30:22.041 Check ok!

2017/03/24/14/30/22/041 Update ATA test flag into Barcode OK.



2017/03/24/14/30/22/044 ÈO,1,OK,E_ATADLL_RESULT_BARCODE_FLAG_OK

2017/03/24/14/30/22/044 DeInit test item object.

2017/03/24/14/30/22/044 Total time cost: 36.04 second. 



2017/03/24/14/30/22/044 Send stop command(AT+STOP) to target.

2017/03/24/14/30/22/208 Release target comm handle.

2017/03/24/14/30/22/218 Release PM comm handle.

2017/03/24/14/30/22/325 Scan barcode not select,use target barcode to rename logfile.
2017/03/24/14/30/22/325 Rename log file (temp2.txt) by barcode: unknown                                                    f
